{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["主机配置"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"主机配置","index":0,"n_rows":12,"n_cols":6,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,4],[2,0,3,0],[4,0,11,0]]}
["配    置"]
[null,null,"CPU","内存","存储","光纤-存储（85T）"]
["中配\n（管理服务器）","server0","2个英特尔至强银牌4214R(2.4GHz/12-Core)","256GB","2个通用硬盘-1200GB","10T"]
[null,"server3","2个英特尔至强银牌4214R(2.4GHz/12-Core)","256GB","2个通用硬盘-1200GB","10T"]
["高配\n（算力）","server2","4个英特尔至强金牌5218(2.3GHz/12-Core)","384GB","5个通用硬盘-2400GB\n2个固态硬盘-480GB"]
[null,"server6","4个英特尔至强金牌5218(2.3GHz/12-Core)","384GB","5个通用硬盘-2400GB\n2个固态硬盘-480GB"]
[null,"server1","4个英特尔至强金牌5218(2.3GHz/12-Core)","384GB","5个通用硬盘-2400GB\n2个固态硬盘-480GB","35T"]
[null,"server4","4个英特尔至强金牌5218(2.3GHz/12-Core)","384GB","5个通用硬盘-2400GB\n2个固态硬盘-480GB","10T"]
[null,"server5","4个英特尔至强金牌5218(2.3GHz/12-Core)","384GB","5个通用硬盘-2400GB\n2个固态硬盘-480GB","20T"]
[null,"server7","4个英特尔至强金牌5218(2.3GHz/12-Core)","384GB","5个通用硬盘-2400GB\n2个固态硬盘-480GB"]
[null,"server8","4个英特尔至强金牌5218(2.3GHz/12-Core)","384GB","5个通用硬盘-2400GB\n2个固态硬盘-480GB"]
[null,"server9","4个英特尔至强金牌5218(2.3GHz/12-Core)","384GB","5个通用硬盘-2400GB\n2个固态硬盘-480GB"]